{{Template}}

|  |
| --- |
| **Appendix** |
|  |

**General Conditions**

* + Analysis Period is Last Six Months or the after the Last Event which ever is later
  + Days with Good Weather (BF<=4) are considered for analysis.
  + Days with Steaming hrs greater than 17 considered for analysis.
  + Data is compared with Original Sea Trial

**Hull Performance**

* + Excess Power < 15 %– Rating Good
  + 15< Excess Power < 25 % – Rating Average
  + Excess Power > 25 % – Rating Poor

**Machinery Performance**

* + SFOC(Grms/kW.hr) within +/- 10 from Shop test condition are considered as "Good"
  + SFOC(Grms/kW.hr) Greater than 10 and less than 20 are considered as "Average"
  + SFOC(Grms/kW.hr) Above 20 are considered as "Poor"